# RF touch switch

Touch switch on ATmega168/328 + nRF24.

## Features

1. Power consumption in sleep mode approximately 10 μA. Up to 2 years of operation on one CR2032 battery (estimated).
2. When triggered transmits battery level charge.
3. Automatic restart in case of a hang-up.
4. Easy installation into any standard touch switch enclosure.

## Note

A gateway is required. For details see [RF Gateway](https://github.com/aZholtikov/RF-Gateway).

Any feedback via [e-mail](mailto:github@zh.com.ru) would be appreciated. Or... [Buy me a coffee](https://paypal.me/aZholtikov).
