# Tested on

1. MOES 1CH 10A. Built on Tuya WiFi module WA2 (WB2S) (BK7231T chip). Replacement required. Performed replacement with ESP-02S (TYWE2S). [Photo](https://github.com/aZholtikov/ESP-NOW-Switch/tree/main/hardware/MOES_1CH_10A).

```text
    Relay GPIO      GPIO04      HIGH
    Led GPIO        GPIO12      LOW
    Button GPIO     GPIO14      RISING
```

2. AUBESS 1CH 16A (Coming soon)
3. LIGHT E27 SOCKET (Coming soon)
