# Tested on

1. MODEL D06 TYPE 1. Built on Tuya WiFi module TYWE3S (ESP8266 chip). Replacement not required. Total triggering time about 1.5 sec. [Photo](https://github.com/aZholtikov/ESP-NOW-Window-Door-Sensor/tree/main/hardware/Model_D06_Type_1).

2. MODEL D06 TYPE 2. Built on Tuya WiFi module CBU (BK7231N chip). Replacement with ESP-M2 (ESP8285 chip). Total response time about 0.5 sec. [Photo](https://github.com/aZholtikov/ESP-NOW-Window-Door-Sensor/tree/main/hardware/Model_D06_Type_2).